## Server 

The server acts as a relay between your Arduino ESP32 device and the STT/LLM/TTS/STS AI Provider API. In ElatoAI, we provide alternative server mechanisms for you to deploy your project globally. 

1. [Deno Edge Functions](https://github.com/akdeb/ElatoAI/tree/main/server/deno) on Deno/Supabase Edge with TypeScript
2. [Cloudflare Workers](https://github.com/akdeb/ElatoAI/tree/main/server/cloudflare) + Durable Objects with TypeScript
3. [FastAPI](https://github.com/akdeb/ElatoAI/tree/main/server/fastapi) with Python (coming soon)
